**CE321 Network Engineering Assignment**

**Dr. M. Reed v5.2**

**Submission details (one document, one Packet Tracer file):**

You will submit a SINGLE word processed document in one of the following formats:

* Word format (.doc or .docx)
* Portable document format (PDF)

You may either edit this document with the required information (and append answers to the parts you are asked to write), or write your own document containing the required information.

Submission should be on Faser by the deadline shown in Faser.

The parts that you need to fill in, or content to append, are:

* Complete the fields in Table 1
* Complete the fields in Table 2
* Include **only** the configurations and **certain** command outputs specified in Task 6.
* Append the explanation for Task 7.

**Additionally,** you must submit your working Packet Tracer file with the **same** configuration as that used for the output given in Task 6.

**You MUST use Packet Tracer 8.0.1 (or later) for this assignment, it is available for download in Windows/Linux/OS X from the CE321 Moodle page. You must use the provided scenario.pkt file available from the CE321 Moodle page.**




**Marks will be awarded as follows (marks in Task 1-6 are in proportion to the correct configuration and documentation):**

* 5% for Task 1 (Table 1 and Table 2)
* 10% for Task 2 (Basic device configuration)
* 35% for Task 3 (OSPF and router features) (of which 15/40 marks are for extension work, see below in Task 3)
* 15% for Task 4 (Switching and VLAN configuration)
* 10% for Task 5 (Access Control Lists)
* 5% for Task 6, Documentation and correct submission of Packet Tracer file.
* 20% for Task 7, Explanation of recovery of routing and switching after failure of primary DS switch (DS1 or DS2). 5/20 of these marks will be for good presentation including use of English and appropriate use of references. See the table in Task 7 for the marking scheme for this task.

**NOTE: this document is a generic description for the whole group. Every student also has a unique combination of IP address ranges, VLAN identifiers and sizes of LANs distributed through the CE321 course pages. Under no circumstances should you use values allocated to another student – doing so will give rise to an investigation of plagiarism. You will find your own individual settings on the CE321 course page using your registration number as a key to your individual page.**

2007 Cisco Systems, Inc. All rights reserved. This document is Cisco Public Information. of



**Figure 1 Assignment topology**

**Scenario**

You are to configure the routing and switching for part of the company network shown in Figure 1, in particular the wide area networking routing (including Branch and Data Centre gateways) and the switching for the Data Centre. Some of the systems are pre-configured. You must complete this assignment using Cisco Packet Tracer version 8.0.1 (or later). Some of the assignment (e.g some IP addresses) is specified exactly, but other parts you will have to make sensible design choices based on the scenario as described here and the methods you have learnt from the lab tasks. You are **highly recommended** to use the version of Packet Tracer available on the Moodle page as it is compatible with that from the laboratory.

You will find that the following devices are already configured and **you should not** change their configuration: InternetServer, ISP, B1, B2, BPC1, DSLink.

You can see the configuration of these devices by either using username and password “donotconfigureme” or by exporting the running configuration from the Config tab. The switches, B1, B2 and DSLink, are just running default switching without any VLANs.

You **must** configure the rest of the devices.

All links are operating at the line speed of their interfaces except for the following:

|  |  |
| --- | --- |
| Network name of link (see Table 1 below) | Line rate |
| DSGW1 (including DSLink) | 100 Mb/s (due to DSLink) cost=1 |
| BRWAN1 | 2 Mb/s cost=50 |
| BRWAN2 | 128 kb/s cost=781 |
| WANDS | 2 Mb/s cost=50 |

The scenario only shows part of the company network, you are to assume that the actual network is very large with many branches (not shown). All the branches connect to the WAN and access the Internet through WAN2.

There is a placeholder for the Internet (InternetServer) accessed through an Internet Service Provider. The router ISP is a placeholder for the Internet Service Providers network. ISP provides one public IP address for the whole company to use (202.202.202.2 on WAN2). The company hosts should be able to access Web servers in the Internet, however, it is not necessary for the Internet to access any hosts in the company network (and in fact the ACLs you will implement will block this traffic).

The data centre needs to have a highly-reliable design and you will note that it has two systems (routers, switches and servers) so that it can cope with a single failure. PC2 is a placeholder for management terminals and only one is shown. There are only two servers and access switches (DS3 and DS4) shown although you should assume there are many more systems to be connected to DS3 and DS4 in the future and not shown. There are no clients or servers directly connected to the distribution layer switches (DS1 and DS2). You should configure the networking so that if there is a failure of any **single** switch, or either router DSR1 or DSR2, then any host will still have network connectivity without any need for manual intervention. You will need to look back at CE231 content to remind you how to allow multiple routers to act as a gateway. (You should assume that DSGW is a highly-fault tolerant router with dual systems and connectivity that are not shown.)

On the Access switches (DS3, DS4), the lower half of the ports (fa0/1-12) are to be allocated to VLAN S, the upper two of the ports (fa0/23-24) are to be allocated to VLAN C. VLAN M is for managing the switches and routers. Other ports are free. All ports not actually connected to a device should be shutdown. VLANs and switch port configuration were covered in CE231.

The company network manager has specified that you use OSPF for routing and to ensure it is configured to route traffic across the whole network and has basic security by limiting where OSPF traffic can be sent/received from to only essential interfaces.

For the OSPF *extension work*:

* OSPF should be reconfigured to be multi-area, the ABRs must be BR1 and DSGW;
* network addresses (routes) between areas must be summarised using a **single** address that is the **smallest** possible summary address to encompass the networks you have been allocated (you are to assume addresses in the summary not used in your scenario are available for expansion at a future date). You will need to find out about this as it is not covered in the Cisco courseware;
* OSPF costs must be correct to allow routing over the fastest path where this is relevant. As the “auto-cost

reference bandwidth” command does not work in Packet Tracer link costs must be set manually.

Note that this extension work will require you to look carefully at the multi-area OSPF Packet Tracer Lab example and to carry out your own research in order to complete it. It is **not** covered by the Cisco courseware in any depth.

**Task 1: Complete the Addressing Scheme.**

The addressing scheme for the network is partially complete, but you will need to allocate the **network addresses** that are blank in Table 1 according to the ranges allocated to you from your individual settings page on Moodle. Fill any blanks or single letters with values that you have been allocated; fill in the WAN addresses marked with “?” using the range allocated to you. Some blank fields will require you to work out suitable values. Any nonapplicable fields marked N/A should not have entries.

Document all subnet addresses in Table 1. **Remember that in Table 1 any interfaces with the same Network**  **Name MUST have the same subnet address! For example BR1 G0/0 and BR3 G0/1 are both connected to BR13 and thus have the same subnet. Make sure this applies to the subnets you are allocating (they have been coloured the same to emphasise that they should be the same subnet.**

**Table 1**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Device** | **Interface** | **Network Number of Name**  **Hosts** | | **Subnet** | **Subnet Mask** |
|  |  | **Branch** | |  |  |
| BR1 | **G0/0** | **BR13** | **2** | **10.1.1.128** | **255.255.255.252** |
| **G0/1** | **BR12** | **2** | **10.1.1.132** | **255.255.255.252** |
| **VLAN 1 (Fa0/1/0)** | **BR1LAN** | **254** | **10.1.36.0** | **255.255.255.0** |
| **S0/0/0** | **BRWAN2** | **2** | **172.16.29.120** | **255.255.255.252** |
| **S0/0/1** | **BRWAN1** | **2** | **172.16.29.124** | **255.255.255.252** |
| BR2 | **G0/1** | **BR12** | **2** | **10.1.1.132** | **255.255.255.252** |
| **G0/0** | **BR23** | **2** | **10.1.1.136** | **255.255.255.252** |
| BR3 | **VLAN 1 (Fa0/1/0)** | **BR3LAN** | **254** | **10.1.0.0** | **255.255.255.0** |
| **G0/1** | **BR13** | **2** | **10.1.1.128** | **255.255.255.252** |
| **G0/0** | **BR23** | **2** | **10.1.1.136** | **255.255.255.252** |
|  |  | **WAN** | |  |  |
| WAN1 | **S0/0/1** | **WANDS** | **2** | **172.16.29.128** | **255.255.255.252** |
| **G0/0** | **WAN12** | **2** | **172.16.29.132** | **255.255.255.252** |
| **S0/0/0** | **BRWAN1** | **2** | **172.16.29.124** | **255.255.255.252** |
| WAN2 | **G0/0** | **WAN12** | **2** | **172.16.29.132** | **255.255.255.252** |
| **G0/1** | **ISP** | **2** | **202.202.202.0** | **255.255.255.252** |
| **S0/0/0** | **BRWAN2** | **2** | **172.16.29.120** | **255.255.255.252** |
|  |  | **ISP and Internet** | |  |  |
| ISP | **G0/0** | **Internet** | **254** | **155.245.0.0** | **255.255.255.0** |
| **G0/1** | **ISP** | **2** | **202.202.202.0** | **255.255.255.252** |
|  |  | **Data Centre** | |  |  |
| DSGW | **S0/0/0** | **WANDS** | **2** | **172.16.29.128** | **255.255.255.252** |
| **G0/0** | **DSGW1** | **2** | **192.168.0.0** | **255.255.255.252** |
| **G0/1** | **DSGW2** | **2** | **192.168.0.4** | **255.255.255.252** |
| DSR1 | **G0/0** | **DSGW1** | **2** | **192.168.0.0** | **255.255.255.252** |
| **G0/1.61** | **DS61** | **254** | **192.168.61.0** | **255.255.255.0** |
| **G0/1.91** | **DS91** | **254** | **192.168.91.0** | **255.255.255.0** |
| **G0/1.121** | **DS121** | **254** | **192.168.121.0** | **255.255.255.0** |
| DSR2 | **G0/0** | **DSGW2** | **2** | **192.168.0.4** | **255.255.255.252** |
| **G0/1.61** | **DS61** | **254** | **192.168.61.0** | **255.255.255.0** |
| **G0/1.91** | **DS91** | **254** | **192.168.91.0** | **255.255.255.0** |
| **G0/1.121** | **DS121** | **254** | **192.168.121.0** | **255.255.255.0** |

Document router/switch interface and PC addresses in Table 2 (these should match the network addresses you assigned in Table 1). Note that interfaces *in italic like this* have already been configured for you. **Make sure where two interfaces are on the same Network you allocate compatible and different IP addresses (again those you are allocating in the same subnet have been coloured the same to help you).**

**Table 2**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Device** | **Interface** | **Network Name** | **IP Address** | **Subnet Mask** | **Gateway** |
| BR1 | ***G0/0*** | ***BR13*** | ***10.1.1.129*** | ***255.255.255.252*** | **N/A** |
| ***G0/1*** | ***BR12*** | ***10.1.1.133*** | ***255.255.255.252*** | **N/A** |
| **VLAN 1 (Fa0/1/0)** | **BR1LAN** | **10.1.36.254** | **255.255.255.0** | **N/A** |
| **S0/0/0** | **BRWAN2** | **172.16.29.121** | **255.255.255.252** | **N/A** |
| **S0/0/1** | **BRWAN1** | **172.16.29.125** | **255.255.255.252** | **N/A** |
| BR2 | ***G0/1*** | ***BR12*** | ***10.1.1.134*** | ***255.255.255.252*** | **N/A** |
| ***G0/0*** | ***BR23*** | ***10.1.1.137*** | ***255.255.255.252*** | **N/A** |
| BR3 | ***VLAN 1 (Fa0/1/0)*** | ***BR3LAN*** | ***10.1.0.254*** | ***255.255.255.0*** | **N/A** |
| ***G0/1*** | ***BR13*** | ***10.1.1.130*** | ***255.255.255.252*** | **N/A** |
| ***G0/0*** | ***BR23*** | ***10.1.1.138*** | ***255.255.255.252*** | **N/A** |
| WAN1 | **S0/0/1** | **WANDS** | **172.16.29.129** | **255.255.255.252** | **N/A** |
| **G0/0** | **WAN12** | **172.16.29.133** | **255.255.255.252** | **N/A** |
| **S0/0/0** | **BRWAN1** | **172.16.29.126** | **255.255.255.252** | **N/A** |
| WAN2 | **G0/0** | **WAN12** | **172.16.29.134** | **255.255.255.252** | **N/A** |
| ***G0/1*** | ***ISP*** | ***202.202.202.2*** | ***255.255.255.252*** | **202.202.202.1** |
| **S0/0/0** | **BRWAN2** | **172.16.29.122** | **255.255.255.252** | **N/A** |
| ISP | ***G0/0*** | ***Internet*** | ***155.245.0.254*** | ***255.255.255.0*** | **N/A** |
| ***G0/1*** | ***ISP*** | ***202.202.202.1*** | ***255.255.255.252*** | **N/A** |
| DSGW | **~~S0/0/1~~ S0/0/0** | **WANDS** | **172.16.29.130** | **255.255.255.252** | **N/A** |
| ***G0/0*** | ***DSGW1*** | ***192.168.0.1*** | ***255.255.255.252*** | **N/A** |
| ***G0/1*** | ***DSGW2*** | ***192.168.0.5*** | ***255.255.255.252*** | **N/A** |
| DSR1 | ***G0/0*** | ***DSGW1*** | ***192.168.0.2*** | ***255.255.255.252*** | **N/A** |
| **G0/1.61** | **DS61** | **192.168.61.1** | **255.255.255.0** | **N/A** |
| **G0/1.91** | **DS91** | **192.168.91.1** | **255.255.255.0** | **N/A** |
| **G0/1.121** | **DS121** | **192.168.121.1** | **255.255.255.0** | **N/A** |
| DSR2 | ***G0/0*** | ***DSGW2*** | ***192.168.0.6*** | ***255.255.255.252*** | **N/A** |
| **G0/1.61** | **DS61** | **192.168.61.2** | **255.255.255.0** | **N/A** |
| **G0/1.91** | **DS91** | **192.168.91.2** | **255.255.255.0** | **N/A** |
| **G0/1.121** | **DS121** | **192.168.121.2** | **255.255.255.0** | **N/A** |
| DS1 | **VLAN 121** | **DS121** | **192.168.121.11** | **255.255.255.0** | **192.168.0.5** |
| DS2 | **VLAN 121** | **DS121** | **192.168.121.22** | **255.255.255.0** | **192.168.0.5** |
| DS3 | **VLAN 121** | **DS121** | **192.168.121.33** | **255.255.255.0** | **192.168.0.5** |
| DS4 | **VLAN 121** | **DS121** | **192.168.121.44** | **255.255.255.0** | **192.168.0.5** |
| InternetServer | ***NIC*** | ***Internet*** | ***155.245.0.1*** | ***255.255.255.0*** | ***155.245.0.254*** |
| BPC1 | ***NIC*** | ***BR3LAN*** | ***10.1.0.1*** | ***255.255.255.0*** | ***10.1.0.254*** |
| BPC2 | **NIC** | **BR1LAN** | **10.1.36.1** | **255.255.255.0** | **10.1.36.254** |
| Server1 | **NIC** | **DS61** | **192.168.61.11** | **255.255.255.0** | **192.168.0.5** |
| Server2 | **NIC** | **DS61** | **192.168.61.22** | **255.255.255.0** | **192.168.0.5** |
| PC2 | **NIC** | **DS91** | **192.168.91.11** | **255.255.255.0** | **192.168.0.5** |

**Task 2: Configure basic device settings.**

Configure the routers and switches that you have been told to configure according to the following guidelines:

* Routers and switches should be secured against unauthorised access and passwords should be stored in a secure manner. Use only the password “cisco” in your configurations.
* There is no DNS server in the network.
* Configure a message-of-the-day banner that warns against unauthorized use and states “This router is managed by 0123456”, where 0123456 is **replaced with your registration number**. • Console input should not be broken with console output messages.
* Any systems that you configure should be capable of being remotely managed using the most secure manner possible. (The systems that you should not configure have not been, and should not be, configured for remote management).

**Task 3: Configure routing and router features.**

Configure the routing and router features to meet the requirements in the scenario using your judgment to make sensible decisions. You should note that the company network is using a private address space that is not allowed to be used in the Internet. These basic OSPF and other routing settings are worth 20/35 of the marks in this task.

***Extension work***

**The extension work is worth 15/35 of the Task 3 marks. While not strictly optional, be aware that you will need to do some self-study and spend some time to complete this part properly.**

This extension work requires you to find out how to implement the multi-area OSPF with correct routing costs as described below, and then implement the features in your scenario. The laboratory experiments or lecture slides do not contain enough detail to show you how to implement them. The features are:

* OSPF should be reconfigured to be multi-area, the area border routers (ABRs) must be BR1 and DSGW;
* network addresses (routes) between areas should be summarised using a single address that is the smallest possible summary address to encompass the networks you have been allocated (you are to assume addresses in the summary not used in your scenario are available for expansion at a future date);
* costs should be correct to allow routing over the fastest path where this is relevant. As the “autocost reference bandwidth” command does not work in Packet Tracer, link costs **must** be set manually to their correct values.

The extension work only requires changes to the OSPF settings, all other settings can be kept the same.

Note that this extension work will require you to look carefully at the multi-area OSPF Packet Tracer Lab example and to carry out your own research in order to complete it. It is not covered by the Cisco courseware in any depth.

**Task 4: Configure switching**

Configure switching as specified in the scenario using your judgement to make sensible decisions.

Configure clients and servers.

Test full connectivity (e.g. company hosts can access the Internet).

**Task 5: Access Control Lists**

Configure ACLs to implement the following policy:

* The whole company network should allow HTTP/HTTPS traffic from the company to the Internet and related HTTP/HTTPS traffic back in. *i.e.*, any company users or systems should be able to browse the Web in the Internet. But all other traffic to/from the Internet should be blocked.
* Traffic should be allowed to move freely within the company network **except** for the following policy for the Branch network which should:
  + allow access to any TCP server in the company network from Branch hosts; o allow users in Branch to browse the Web in the Internet (as specified in the first policy point);
  + allow PC2 (a system administrator) to connect to any hosts in Branch using SSH to manage the systems;
  + allow any OSPF traffic;
  + block any other traffic *i.e.*, systems outside of Branch should not be able to initiate TCP connections into Branch.

**Task 6: Document *certain* specified parts of the configurations and include in your submitted document.**

You **must not** include all the running configurations in your submitted document. Instead you should **only show the items below from the running configurations:**

* the “router OSPF” block of the running configuration for the routers DSGW and BR1 o *i.e.*, the router block from the output show running-config | begin router

DSGW:

router ospf 1

router-id 0.0.1.1

log-adjacency-changes

area 1 range 192.168.0.0 255.255.0.0

network 192.168.0.0 0.0.0.3 area 1

network 192.168.0.4 0.0.0.3 area 1

network 172.16.29.128 0.0.0.3 area 0

! This ospf block has the networks connected to DSGW with specified areas, and router-id; also it summarizes the ospf area 1 as DSGW is the ABR for area 1, and we can see the summarized route from any other router outside area 1.

BR1:

router-id 0.0.2.1

log-adjacency-changes

area 2 range 10.1.0.0 255.255.192.0

passive-interface Vlan1

network 10.1.1.128 0.0.0.3 area 2

network 10.1.1.132 0.0.0.3 area 2

network 10.1.36.0 0.0.0.255 area 2

network 172.16.29.120 0.0.0.3 area 0

network 172.16.29.124 0.0.0.3 area 0

! This ospf block has the networks connected to BR1 with specified areas, passive interface ,and router-id; also it summarizes the ospf area 2 as BR1 is the ABR for area 2, and we can see the summarized route from any other router outside area 2.

* interface specifications for configured interfaces on routers DSR1 and DSR2 o *i.e.*, the interface settings from show running-config | begin interface

DSR1:

interface GigabitEthernet0/0

description Network DSGW1

ip address 192.168.0.2 255.255.255.252

duplex auto

speed auto

!

interface GigabitEthernet0/1

no ip address

duplex auto

speed auto

!

interface GigabitEthernet0/1.61

description Network DS61 VLAN61

encapsulation dot1Q 61

ip address 192.168.61.1 255.255.255.0

standby 61 ip 192.168.61.254

!standby router in VLAN 61 network

!

interface GigabitEthernet0/1.91

description Network DS91 VLAN91

encapsulation dot1Q 91

ip address 192.168.91.1 255.255.255.0

standby 91 ip 192.168.91.254

!standby router in VLAN 91 network

!

interface GigabitEthernet0/1.121

description Network DS121 VLAN121

encapsulation dot1Q 121

ip address 192.168.121.1 255.255.255.0

standby 121 ip 192.168.121.254

!standby router in VLAN 121 network

!

DSR2:

interface GigabitEthernet0/0

description Network DSGW2

ip address 192.168.0.6 255.255.255.252

duplex auto

speed auto

!

interface GigabitEthernet0/1

no ip address

duplex auto

speed auto

standby version 2

!

interface GigabitEthernet0/1.20

no ip address

shutdown

!

interface GigabitEthernet0/1.60

no ip address

shutdown

!

interface GigabitEthernet0/1.61

description Active router in network DS61( VLAN61 )

encapsulation dot1Q 61

ip address 192.168.61.2 255.255.255.0

standby 61 ip 192.168.61.254

standby 61 priority 150

standby 61 preempt

!

interface GigabitEthernet0/1.91

description Active router in network DS91( VLAN91 )

encapsulation dot1Q 91

ip address 192.168.91.2 255.255.255.0

standby 91 ip 192.168.91.254

standby 91 priority 150

standby 91 preempt

!

interface GigabitEthernet0/1.121

description Active router in network DS121( VLAN121 )

encapsulation dot1Q 121

ip address 192.168.121.2 255.255.255.0

standby 121 ip 192.168.121.254

standby 121 priority 150

standby 121 preempt

!

* the complete running configuration of WAN2 o *i.e.,* the output of show running-config

WAN2(config)#do show run

Building configuration...

Current configuration : 2211 bytes

!

version 15.1

no service timestamps log datetime msec

no service timestamps debug datetime msec

no service password-encryption

!

hostname WAN2

!

!

!

enable secret 5 $1$mERr$hx5rVt7rPNoS4wqbXKX7m0

!

!

!

!

!

!

no ip cef

no ipv6 cef

!

!

!

username cisco secret 5 $1$mERr$hx5rVt7rPNoS4wqbXKX7m0

!

!

license udi pid CISCO1941/K9 sn FTX1524HP87

!

!

!

!

!

!

!

!

!

no ip domain-lookup

ip domain-name cisco

!

!

spanning-tree mode pvst

!

!

!

!

!

!

interface GigabitEthernet0/0

ip address 172.16.29.134 255.255.255.252

ip nat inside

duplex auto

speed auto

!

interface GigabitEthernet0/1

description !! ip route 202.202.202.2 255.255.255.252 202.202.202.1 (Q)

ip address 202.202.202.2 255.255.255.252

ip access-group BROWSING in

ip access-group SURFING out

ip nat outside

duplex auto

speed auto

!

interface Serial0/0/0

ip address 172.16.29.122 255.255.255.252

ip nat inside

clock rate 2000000

!

interface Serial0/0/1

no ip address

clock rate 2000000

shutdown

!

interface Serial0/1/0

no ip address

clock rate 2000000

shutdown

!

interface Serial0/1/1

no ip address

clock rate 2000000

shutdown

!

interface Vlan1

no ip address

shutdown

!

router ospf 1

router-id 0.0.0.2

log-adjacency-changes

area 0 range 172.16.29.0 255.255.255.0

network 172.16.29.132 0.0.0.3 area 0

network 172.16.29.120 0.0.0.3 area 0

network 202.202.202.0 0.0.0.3 area 0

default-information originate

!

ip nat inside source list SURFING interface GigabitEthernet0/1 overload

ip classless

ip route 0.0.0.0 0.0.0.0 GigabitEthernet0/1

!

ip flow-export version 9

!

!

ip access-list extended SURFING

remark Permits inner users to surf the internet

permit tcp any any eq www

permit tcp any any eq 443

deny ip any any

ip access-list extended BROWSING

remark Permits HTTP & HTTPS protocols from the internet to inner network

remark Permits HTTP & HTTPS protocols from the internet to inner network, and deny all other traffic

permit tcp any eq www any

permit tcp any eq 443 any

deny ip any any

!

no cdp run

!

banner motd ^C This router is managed by 1906184^C

!

!

!

!

!

line con 0

logging synchronous

!

line aux 0

!

line vty 0 4

login local

transport input ssh

line vty 5 15

login local

transport input ssh

!

!

!

end

* any ACLs by specifying the router they are running on and showing the ACLs and the relevant interface configurations
  + to show interfaces config use show running-config | begin interface o

to show ACLs use show running-config | begin access-list

BR1:

interface GigabitEthernet0/0

ip address 10.1.1.129 255.255.255.252

ip access-group STDIN in

ip access-group STDIN out

duplex auto

speed auto

!

interface GigabitEthernet0/1

ip address 10.1.1.133 255.255.255.252

ip access-group STDIN in

ip access-group STDIN out

duplex auto

speed auto

!

interface Serial0/0/0

ip address 172.16.29.121 255.255.255.252

ip ospf cost 781

ip access-group STDIN in

ip access-group STDIN out

!

interface Serial0/0/1

ip address 172.16.29.125 255.255.255.252

ip ospf cost 50

ip access-group STDIN in

ip access-group STDIN out

!

interface Vlan1

description BR1LAN (needs configuring with IP address 10.1.L.254

ip address 10.1.36.254 255.255.255.0

ip access-group STDIN in

ip access-group STDIN out

!

ip access-list extended STDIN

remark This ACL is for blocking all traffic except OSPF, and SYSADMIN PC2

permit ospf any any

permit tcp any eq www any

permit tcp any eq 443 any

remark This ACL is to permit internet, OSPF, TCP servers and, SYSADMIN PC2 only, and block all other traffic

permit tcp host 192.168.91.11 any eq 22

permit tcp any eq 22 host 192.168.91.11

permit tcp 192.168.61.0 0.0.0.255 any

permit tcp any 192.168.61.0 0.0.0.255

permit tcp any any eq www

permit tcp any any eq 443

!

DSGW(config)#do show run | begin interface

interface GigabitEthernet0/0

ip address 192.168.0.1 255.255.255.252

ip access-group STDINOUT in

ip access-group STDINOUT out

duplex auto

speed auto

!

interface GigabitEthernet0/1

ip address 192.168.0.5 255.255.255.252

ip access-group STDINOUT in

ip access-group STDINOUT out

duplex auto

speed auto

!

interface Serial0/0/0

ip address 172.16.29.130 255.255.255.252

ip access-group STDINOUT in

ip access-group STDINOUT out

clock rate 2000000

!

DSGW(config)#do show run | begin access-list

ip access-list extended STDINOUT

permit ospf any any

permit tcp any eq www any

permit tcp any eq 443 any

permit tcp host 192.168.91.11 any eq 22

permit tcp any eq 22 host 192.168.91.11

permit tcp any any eq www

permit tcp any any eq 443

remark This ACL is to block all traffic in the network except SYSADMIN PC2, TCP servers, OSPF, and Internet http & https

permit tcp 192.168.61.0 0.0.0.255 any

permit tcp any 192.168.61.0 0.0.0.255

deny ip any any

!

WAN2(config)#do show run | begin interface GigabitEthernet0/1

interface GigabitEthernet0/1

description !! ip route 202.202.202.2 255.255.255.252 202.202.202.1 (Q)

ip address 202.202.202.2 255.255.255.252

ip access-group BROWSING in

ip access-group SURFING out

ip nat outside

duplex auto

speed auto

!

WAN2(config)#do show run | begin access-list

ip access-list extended SURFING

remark Permits inner users to surf the internet

permit tcp any any eq www

permit tcp any any eq 443

deny ip any any

ip access-list extended BROWSING

remark Permits HTTP & HTTPS protocols from the internet to inner network

remark Permits HTTP & HTTPS protocols from the internet to inner network, and deny all other traffic

permit tcp any eq www any

permit tcp any eq 443 any

deny ip any any

!

Additionally, you **must** show the output of the following command:

* the output of show ip route on DSGW and BR1

DSGW(config)#do show ip route

Codes: L - local, C - connected, S - static, R - RIP, M - mobile, B - BGP

D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area

N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2

E1 - OSPF external type 1, E2 - OSPF external type 2, E - EGP

i - IS-IS, L1 - IS-IS level-1, L2 - IS-IS level-2, ia - IS-IS inter area

\* - candidate default, U - per-user static route, o - ODR

P - periodic downloaded static route

Gateway of last resort is 172.16.29.129 to network 0.0.0.0

10.0.0.0/18 is subnetted, 1 subnets

O IA 10.1.0.0/18 [110/129] via 172.16.29.129, 00:45:27, Serial0/0/0

172.16.0.0/16 is variably subnetted, 5 subnets, 2 masks

O 172.16.29.120/30 [110/129] via 172.16.29.129, 00:46:12, Serial0/0/0

O 172.16.29.124/30 [110/128] via 172.16.29.129, 00:46:52, Serial0/0/0

C 172.16.29.128/30 is directly connected, Serial0/0/0

L 172.16.29.130/32 is directly connected, Serial0/0/0

O 172.16.29.132/30 [110/65] via 172.16.29.129, 00:46:12, Serial0/0/0

192.168.0.0/24 is variably subnetted, 4 subnets, 2 masks

C 192.168.0.0/30 is directly connected, GigabitEthernet0/0

L 192.168.0.1/32 is directly connected, GigabitEthernet0/0

C 192.168.0.4/30 is directly connected, GigabitEthernet0/1

L 192.168.0.5/32 is directly connected, GigabitEthernet0/1

O 192.168.61.0/24 [110/2] via 192.168.0.6, 00:46:22, GigabitEthernet0/1

[110/2] via 192.168.0.2, 00:46:22, GigabitEthernet0/0

O 192.168.91.0/24 [110/2] via 192.168.0.6, 00:46:22, GigabitEthernet0/1

[110/2] via 192.168.0.2, 00:46:22, GigabitEthernet0/0

O 192.168.121.0/24 [110/2] via 192.168.0.6, 00:46:22, GigabitEthernet0/1

[110/2] via 192.168.0.2, 00:46:22, GigabitEthernet0/0

202.202.202.0/30 is subnetted, 1 subnets

O 202.202.202.0/30 [110/66] via 172.16.29.129, 00:46:12, Serial0/0/0

O\*E2 0.0.0.0/0 [110/1] via 172.16.29.129, 00:46:42, Serial0/0/0

BR1(config)#do show ip ro

Codes: L - local, C - connected, S - static, R - RIP, M - mobile, B - BGP

D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area

N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2

E1 - OSPF external type 1, E2 - OSPF external type 2, E - EGP

i - IS-IS, L1 - IS-IS level-1, L2 - IS-IS level-2, ia - IS-IS inter area

\* - candidate default, U - per-user static route, o - ODR

P - periodic downloaded static route

Gateway of last resort is 172.16.29.126 to network 0.0.0.0

10.0.0.0/8 is variably subnetted, 8 subnets, 3 masks

O 10.1.0.0/24 [110/2] via 10.1.1.130, 00:47:16, GigabitEthernet0/0

C 10.1.1.128/30 is directly connected, GigabitEthernet0/0

L 10.1.1.129/32 is directly connected, GigabitEthernet0/0

C 10.1.1.132/30 is directly connected, GigabitEthernet0/1

L 10.1.1.133/32 is directly connected, GigabitEthernet0/1

O 10.1.1.136/30 [110/2] via 10.1.1.134, 00:47:16, GigabitEthernet0/1

[110/2] via 10.1.1.130, 00:47:16, GigabitEthernet0/0

C 10.1.36.0/24 is directly connected, Vlan1

L 10.1.36.254/32 is directly connected, Vlan1

172.16.0.0/16 is variably subnetted, 6 subnets, 2 masks

C 172.16.29.120/30 is directly connected, Serial0/0/0

L 172.16.29.121/32 is directly connected, Serial0/0/0

C 172.16.29.124/30 is directly connected, Serial0/0/1

L 172.16.29.125/32 is directly connected, Serial0/0/1

O 172.16.29.128/30 [110/100] via 172.16.29.126, 00:47:56, Serial0/0/1

O 172.16.29.132/30 [110/51] via 172.16.29.126, 00:47:26, Serial0/0/1

O IA 192.168.0.0/16 [110/101] via 172.16.29.126, 00:46:31, Serial0/0/1

202.202.202.0/30 is subnetted, 1 subnets

O 202.202.202.0/30 [110/52] via 172.16.29.126, 00:47:26, Serial0/0/1

O\*E2 0.0.0.0/0 [110/1] via 172.16.29.126, 00:47:26, Serial0/0/1

For the first **four** items above (the parts of the running configurations), add comments describing the significant features in the configuration using the “!” symbol at the start of a comment line and by using the description command for all interfaces and a remark for ACLs.

The configurations and command output should be in a fixed width font such as this. If you are simply using this document as a template you can paste the necessary output here (with a suitable title before each one).

**IT IS VITAL THAT YOUR PACKET TRACER FILE CONTAINS THE SAME**

**CONFIGURATIONS THAT YOU SUBMIT IN THE DOCUMENT. ANY FAILURE TO DO SO**

**WILL MEAN ZERO MARKS FOR THE DOCUMENTATION PART AND THE MARKER**

**MAY TAKE THE LOWER OF THE FUNCTIONALITY IN EITHER OF THE**

**CONFIGURATIONS. IF YOU SIMPLY DUMP WHOLE CONFIGURATIONS, NOT IN THE LIST ABOVE, IN YOUR SUBMITTED DOCUMENT YOU WILL SCORE ZERO FOR DOCUMENTATION.**

**Task 7: Explain switching and routing recovery after failure of either switch DS1 or DS2**

You have implemented a resilient design in the Data Centre. If either switch DS1 or DS2 fails it should still be possible for an external host such as BPC1 to contact a server without any manual intervention.

From Server 1 ping WAN2 (or another device outside the Data Centre) and determine which **router** (DSR1 or DSR2) is used to send the packet beyond the Data Centre using your design. Once you have determined this you must consider what happens when the neighbouring switch fails; *i.e.* if DSR1 is the router to send the packet to DSGW then consider what happens when DS1 fails.

Describe the recovery from failure by explaining how the routers and switches handle the failure. You should describe the protocols that are used to recover from the failure and how they operate **in the context of your network**. You do not need to give details of exact messages as there are too many involved; however, you should explain in general terms the messages needed to recover from the failure.

It is recommended that you attempt this part even if you do not have a complete network design. You will still receive marks for the description.

You should aim for approximately two sides for this explanation (not including any diagrams) and it should not contain unnecessary background information. It should read as a self-contained document and have a suitable structure (i.e. an introductory paragraph and a closing paragraph). You **must** use references for sources that support your description and would give more information to the reader – an example might be the standards documents for protocols (e.g. RFCs) and/or a textbook. **Web references are not suitable.** However, IETF RFC’s are allowed (even though they are normally distributed via the web).

|  |  |
| --- | --- |
| Mark Task 7 | Task 7 Guideline attributes |
| 100% (20/20) | Full description in the switching and routing layers of the recovery after failure. The necessary protocols are fully described using examples from the network. The description is written to a professional standard with excellent grammar and has full list of citations to authoritative sources for each system or protocol. |
| 70% (14/20) | A good description in the switching and routing layers of the recovery after failure. The necessary protocols are described in some depth using examples from the network. The description is written to a professional standard with good grammar and has good list of citations to authoritative sources. |
| 60% (12/20) | A good description in the switching and routing layers of the recovery after failure including the necessary protocols using examples from the network; although one of the protocols or systems may be described in less depth. The description is written to a reasonable standard with reasonable grammar and has a list of citations to authoritative sources. |
| 50% (10/20) | A description in the switching and/or routing layers of the recovery after failure with some protocols described using examples from the network. The description is written to a reasonable standard but with some grammatical errors, some citations to, mostly, authoritative sources are given. |
| 40% (8/20) | A description in the switching or routing layers of the recovery after failure with at least one protocol described using examples from the network. The description is |
|  | written to an acceptable standard but with some grammatical errors, some citations are given. |
| <40% (<8/20) | A failure to describe even one of either the switching or routing layers used for recovery after failure. |

**Marking Descriptors for Task 7**

**End of Assignment**